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PRAVEEN KUMAR.U

Email:
prvnkumar1988@gmail.com

Skype ID: live:prvnkumar1988_1

Permanent Address :
POYIKAKKARAYIL                                                                                                                     
KS PURAM  .P. O.
KOLLAM– 690544
KERALA
INDIA
       
[bookmark: _Toc44005438]Personal Data:  
Father’s Name  :    K.UTHAMAN
Date of Birth     :   17/01/1989
Age                   :    32 yrs
Gender              :    Male
Marital Status   :    Married 
Nationality        :    Indian

Phone
Mob: +968 94041724
Imo :- +91 8137839399

Vaccination Details:  
Vaccine name  : Covishield (   Oxford -AstraZeneca )
Vaccination status : Fully vaccinated
First dose date :  08-Aug-2021
Second dose date :  16-Sep-2021





	 Career Objective

To present in very challenging environment, that will enable me to expand my areas of responsibilities and actively participate as team member to contribute the growth of the company.
  Personal Strength
· Having pleasing personality and very good interpersonal skills.
· Energetic, young, dedicated, self-motivated and a through approach to work
· Capable of working own initiative.
· Ability to adapt to new environments.
· Ability to lead effectively under pressure to attain specified goals.
· Excellent command of communication of English language.
· Ability to organize, co-ordinate, implemented control over work related activities.
· Strong supervisory experience in electrical maintenance.
· Strong knowledge of preventive maintenance activities.
  Educational Qualifications 
	BTech Electrical engineering
(2007-2011)
	
Total marks-61%
	
2011

	Postgraduate diploma in industrial automation 
	
Level-1
	
2013

	Vocational higher secondary (2004-2006)
	
Total marks -79%
	
2006

	
SSLC (2004)
	
Total marks -75%
	
2004






 





JOB PROFILE

	Company
	BEC OMAN
(FACILITY / ELECTRICAL MAINTENANCE)

	Position
	MAINTENANCE ENGINEER (Shutdown)

	Duration
	17-DEC-2021 TO 16-FEB-2022
(TOTAL EXPERIENCE 2 MONTHS)

	· Electrical maintenance of MOD facilities in Oman.
·  Electrical maintenance of substations and RMU units.
· Electrical maintenance of diesel / gas power plants
· Lockout-tagout of MV & LV Panels for shutdown maintenance 
· Preventive maintenance / condition monitoring of underground cables, transformers, and switch gears.
· Allocation of manpower including Forman’s and technicians for shutdown maintenance.

	Company
	YOL MILITARY STATION 
(ENERGY AUDITING, FACILITY / ELECTRICAL MAINTENANCE)

	Position
	MAINTENANCE ENGINEER (Two-year contract)

	Duration
	10-OCT-2019 TO 10-MAY-2021
(TOTAL EXPERIENCE 2 YEARS)

	· Electrical maintenance of military office, residential apartments, and recreation facilities.
·  Electrical maintenance of 33KV MIS substation, 11 / 0.415 KV cabin substations, 11KV RMU units and LV overhead lines.
· Electrical maintenance of solar power plant which includes 500 KW solar power plant and its battery bank.
· Yearly Energy auditing of station facilities.
· Lockout-tagout of MV & LV Panels for shutdown maintenance 
· Preventive maintenance / condition monitoring of underground cables, transformers, and switch gears.
· Allocation of manpower including Forman’s and technicians for regular maintenance.

	Company
	SHAHER UNITED TRADING AND CONTRACTING COMPANY                                                                           (Petroleum Development Oman contractor, PDO 132KV Transmission maintenance contract, Contract no: C31/1636 )
(PREVENTIVE AND CORRECTIVE MAINTENANCE OF PDO SUBSTATIONS AND POWER STATIONS)

	Position
	ELECTRICAL MAINTENANCE SUPERVISOR  

	Duration
	04-JULY-2013 TO 29-Septemper-2019
(TOTAL EXPERIENCE 6 YEARS & 2 MONTHS)

	Corrective maintenance

· Maintenance of Power plant transformer, Substations and OHL up to 132KV (Petroleum development Oman south oil field)

· Trouble shooting of electrical equipment’s such as Power and Auxiliary Transformers, Circuit breakers, Isolators, Battery chargers, Battery banks and ups systems.

· Switching operation of substations up to 132KV with AEP / SAEP

· Electrical maintenance in special zone EPZ areas (Petroleum development Oman High sour areas [H2S] -Harweel, Birba and Al Noor) 

· Holder of PDO authorizations such as Competent electrical person (ESR No:   E 98857962) and Permit to Work (License No: 5494) 

· GIS Switching operation of outdoor (132KV Pole type) and indoor integrated Circuit breakers up to 33KV (ABB, Schneider…….)

· Filling of SF6 gas on GIS switch gear by using portable device such as DILO R115 

· Trouble shooting of explosion / flame proof LV motors up to 55 KW (Single frame type, Ex de) by conducting winding insulation test, Thermography inspection, …etc 

· Maintenance of Circuit breakers both Medium and Low voltage (Type- ACB, VCB, MCCB …etc.)

· Tan delta test for transformers, motors, and cables……

· Hi-pot test for transformers, cables, and surge arrestors.

· Maintenance of substation auxiliaries such as DC chargers, UPS, and DG panels

· Lock out and tag out of LV AC and DC Distribution system

Condition monitoring / Preventive maintenance 

· Authorized electrical inspector for Preventive maintenance activities such as Thermography inspection, Partial discharge, and Corona inspection for PDO Generation, Transmission, Production, Terminal stations and Steam power plants. (Authorized by PDO-UIE3Y)

· Completed Level-1 Thermographic inspection.

· Completed Level-1 Partial discharge Test.

· Completed Level -1 Corona inspection.

· Thermographic inspection of Switch yards and substations up to 132KV (Transformers, CT, VT, CVT, CB, Isolators’…etc.) 
Instrument used: Visir 640, Company: Thermoteknix, UK
Instrument used: Flir T 1020, Company: Flir, UK
Instrument used: Fluke TiX 580, Company: Fluke, UK

· Thermographic inspection of UPS and Battery chargers (UPS Model-Chloride, snichder and Gutor, Battery charger-HBL

· Online / offline Partial discharge test for Transformers, switchgears, Motors and HV Cables up to 132kv
Instruments used: HVPD Kronos (GIS Switch gear partial discharge Test- UHF Barrier sensor / UHF sensor node), HVPD Long shoot, HVPD PDS Air (Test-HFCT, TEV, Ultrasonic and Air born Acoustic)
Company: HVPD, UK
Instrument used: PD monitor (Test-Ultrasonic and TEV-Transient earth voltage)
Company: EA technologies, UK

· Corona inspection of Switch yards and Overhead lines up to 132KV
Instruments: Crocam 504, Corocam 7, Company: Coronacam TM, UK

· Detection of gas leakage in gas wells, pipelines and gas plants / process area using Flir GFX 320 OGI thermal imaging camera.  (For supporting Crude / gas process engineers)
            Instruments: Flir GFX 320, Company: Teledyne Flir

· Thermal mapping-Thermographic inspection of Crude Oil Separator Tanks, Storage Tanks, Vessels, Pipeline flanges and valves, gas storage tank, gas separator tank, gas compressors for finding gas leakage and sludge formation in Crude oil and gas production stations. (For supporting Crude / gas process engineers)
Instrument used: Visir 640, Company: Thermoteknix, UK
Instrument used: Flir T 1020, Company: Flir, UK

· 3Y PM (Load test) of substation and power station battery bank by using Torkel 860 and DV Power BLU360V discharge kits (Chloride, HBL, Gutor, Borri , Schneider……………).


Testing
· Experience in testing of transformer, switch gear, Cable, battery bank, DC chargers and UPS up to 1200 Ah. (Working under testing and commissioning engineer)

Transformer testing 
· Transformer insulation testing (Tan delta)
Instrument used: Delta 4000 series (12Kv insulation diagnostic systems
Company: - Megger, UK, Software: - Power DB 
· Transformer three phase ratio and winding resistance analyzer 
Instrument used: MWA 300, Company: - Megger, UK, Software: - Power DB 
· Transformer insulating oil testing / dielectric strength test  
Instrument used: OTS80PB, Company: - Megger, UK

Switch gear testing 
· Circuit breaker time travel analysis /Timing test 
Instrument used: EGIL (Circuit breaker analyzer), Company: - Megger, UK
Software: - CABA Win (Circuit breaker analysis software) 
· Circuit breaker contact resistance test / Ductor test 
Instrument used: DLRO  600, Company: - Megger, UK
· Circuit breaker insulation test  
Instrument used: Delta 4000 series (12Kv insulation diagnostic systems)
Company: - Megger, UK, Software: - Power DB 
HV cable Testing 
· HV cable Testing 
5KV / 10KV insulation test for cables,100KV 50HZ Test system (High pot test) 
Instruments used: MIT 1025 and HPA 100 AC & HPA 100 DC 
Company: - Megger, UK
Battery bank load test of DC charger / UPS 
· Load testing / efficiency testing of battery bank by using DV power discharge kit / Torkel 860 discharge kit
Instruments used: DVB 360V (Discharge kit), DVB 360U (Extended load) and Torkel 860 (Discharge kit)
            Company: - Megger, UK, Software: - DV-B Win 

Earth testing / Ground resistance checking 
· Ground resistance checking to ensure effective earthing system
Instrument used: Erath electrode resistance tester, DET3TD, Company: - Megger, UK

Hot Stick / Wet stick testing 
· Hot stick wet stick testing to ensure insulation level / insulation degradation 
Instrument used: Hot stick / Wet stick tester, C403-3179 (230 Volts)
Company: - HUBBELL / CHANCE, UK

SF6 Gas leak detection  
· SF6 gas leak detection for gas insulated switch gear up to 132KV
Instrument used: DILO Gas leak detector, DILO 3-033-R002, Company: - DILO, USA

SF6 Gas handling (Filling / Evacuation)  
· SF6 gas handling (Filling / Evacuation) for gas insulated switch gear (Pole & Modular type) up to 132KV
Instrument used: DILO Gas handling unit, B143R11, Company: - DILO, USA

Live line washing of insulators and switch yard equipment up to 132KV

            Live line washing
· Live line washing of overhead line insulators and switch yards equipment up to 132KV by using DM water and Live line washing skid (IW-SD 2000L with auto trip function) (Overhead line insulators, Transformer bushing, Outdoor cable terminations, Outdoor circuit breakers….)
· Pre-work verification or disabling of auto reclosers and circuit breakers up to 132KV.
· Pre- work inspection of live line washing skid 
· Verification of skid platform and nozzle earthing (visual / Earth megger)
· Verification of auto trip function of washing skid motor (DM water conductivity / Temperature)
·  Manual verification of DM water by using conductivity meter
· Verification of continuous pressure of washing skid motor
· Verification of wind speed by using anemometer

	Company
	TECNOMARK ENGINEERS INDIA Pvt.Ltd.
(MEP, ENERGY MANAGEMENT, POWER T&D, MAINTENANCE)

	Position
	JUNIOR MAINTENANCE ENGINEER

	Duration
	01-SEPT-2011 TO 17-MAY-2013
(TOTAL EXPERIENCE 1 YEAR AND 8 MONTHS)

	· Plant operation :-(Comprising of 4MVA TF, 3NOS 1600KVA TF’S, 33KV MV PANEL and 2 Nos of LV PANEL.)
· Checking and fixing problems with electrical panels and machines.
· Lockout-tagout of MV & LV Panels for shutdown maintenance 
· Troubleshooting of motors and motor starters 
· Testing of transformers up to 1600KVA (Voltage ratio, insulation and BDV test.
· Preventive maintenance / condition monitoring of underground cables, motors, transformers and MV switch gears.
· Load test of battery bank by using Torkel 860 discharge kits.
· Monthly Thermographic inspection of motors, transformers, switch gears and generators for checking the thermal variations.
              Instrument used: Fluke TIS20


Software’s 
Power DB Pro: - Megger Acceptance & Maintenance test data management software 
CABA Win: - Circuit breaker analysis software
DV-B Win: - Battery load test / efficiency test of DC charger / UPS 
Thermoteknix-IR reporter and IR analyzer tools 
Flir Tools +   -Thermal image reporter and analyzer
Flir Report Studio- Thermal image templates creator / New report format creator 
Fluke connect - Thermal image reporter and analyzer
HVPD -PDS Gold (Partial discharge analyzing and reporting software)
ETAP-Electrical transient analyzer program ver5.5.6 
Operating Systems: -Windows
SAP: - Basic knowledge in SAP software                                                                    
TRAINING / COURSE 
· Successfully completed all the mandatory Safety courses such as First aider, Authorized gas tester and other courses as per the PDO requirement.
· Successfully completed Live line maintenance training from PDO (Pacific Gas & Electric Co., USA) 
· Attended VHSE on job training conducted by INDIAN RARE EARTHS LIMITED
· Attended industrial training in hydroelectric project at Pallivasal, Munnar
· Training in industrial automation by PROLIFIC SYSTEMS & TECHNOLOGIES LIMITED
· Attended short term course on ETAP conducted by KLG SYSTEL LIMITED

Passport Details
Passport No      :   V3060345
Date of Reissue :   28-10-2021
Date of Expiry	  :   27-10-2031	 

Languages known

· English
· Arabic
· Malayalam

Oral fluency: English, Arabic, Malayalam 
Written fluency: English, Malayalam                                                                                 
Declaration
             I hereby certify that the above made statements are true to the best of my knowledge.

Date: 18-02-2022
Place:  Kerala, India                                                                               PRAVEEN KUMAR UTHAMAN
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