CURRICULUM VITAE
POST APPLIED FOR		        :  MECHANICAL TECHNICIAN				
NAME IN FULL			: PATEL RAJUBHAI RAMABHAI
Address				: At & Po. Danti, (Jalaram Street)
					  Via : Maroli Bazar, Ta. Jalalpore,
					  Dist : Navsari, Gujarat State, INDIA
					  Pin  Code : 396 436 ( e mail- raju291972@yahoo.com )
Contact No.				: +919601823178, +918401661521
Date & Place of Birth		: 29-12-1978   Danti ( Navsari)
Nationality				: Indian
Marital Status			: Married
Languages Known			: English, Hindi and Gujarati.


DETAIL OF PASSPORT		:-EMIGRATION STATUS (ECNR)
                                              Passport  No. : M 0947659  Issue At : Surat
                                              Issue Date	:  19-08-2014   Expiry on  : 18-08-2024  	

EDUCATION  QUALIFICATION  : Passed New S.S.C. Exam Board of Gujrat.

TECHNICAL QUALIFICATION    : Diploma in Mechanical Engineering

EXPERIENCE	: IN OVERSEAS Offshore Oil & Gas Plant, Refinery, Petrochemicals, Fertilizer, LNG Plant, maintenance and commissioning job
	
	Company name 
	Duration 
	Designation 

	· 
	M/S Manweir Co. Siemens Energy Supply Qatar SHELL utility and F.G.P. Shutdown Doha Qatar
	07-01-2022 to 08-03-2022
	Rotating Technician

	· 
	M/S ERAM CO. MHIPOWER SUPPLY ADNOC FERTIL-1 SHUTDOWN, ABU DHABI
	20-10-2021 to 21-11-2021
	Mechanical Technician

	· 
	M/S EMDAD Co. At ADNOC Takreer  Refinery (WEST ) RRW Shut Down , ABU DHABI.
	10-01-2019 to 10-08-2019
	Mechanical Technician.

	· 
	M/s.ANABEEB Co.At Al Bayroni FERTILIZER IBN Zahr and SIPCHEM Shutdown Saudi Arabia.
	22-01-2018 to 05-11-2018
	Rotary Tech.

	· 
	M/s.SPARK Co.at ZADCO ADNOC OFFSHORE Shutdown Satah Plant Abu-Dhabi.
	24-09-2017 to 09-11-2017
	Mechanical Technician.

	· 
	M/s. Gulf Energy Co. at QAFCO Fertilizer shutdown and Qatar steel shutdown DOHA QATAR.
	21-10-2016 to 19-01-2017
	Mechanical Tech.

	· 
	M/s. ALshirah co. at ADNOC Takreer  Refinery (EAST ) shutdown, Abu dhabi, UAE
	03-02-2016 to 27-03-2016

	Millwright Technician 

	· 
	M/s ABC Recruitment Co.at ADGAS Das Island. Abu Dhabi Train 3 ,Train 1&2 with Storex Jetty Shut down .Das Island Abu Dhabi.
	28-10-2013 to 31-12-2014
	 Mechanical Tech.

	· 
	Ms QNFS (Flour) at Qatar Shell GTL,Phase-1 & 2, Doha Qatar
	22-08-2012 to 23-05-2013
	 Mechanical Tech.

	· 
	Ms. S.T.S. Co AT ORPIC Refinery Shutdown Oman (Muscat)
	15 – 03 -  2012  to  27- 04 - 2012
	Rotating Equip. Mech.

	· 
	M/s. C.T.S. Co. at Habshan Gasco -Bab Gasco and Buhasa Gasco with Ruwais Gasco plant   shut down Abu Dhabi
	09-03-2010 to 08-07-2011
	. Mechanical Tech.

	· 
	M/s. Al Melehy Trading at ADMA Opco Offshore Survival safety training Course, Umm Shaif S.C. G.T.P. and N.G.T.P.  Abu Dhabi.
	16-03-2007 t0 08-11-2009
	Mech. Fitter

	· 
	M/s. Tespec Co. at Gasco Ruwais Plant -1 Shutdown Frist aid Awareness Training Course, 2007 On Shore, Abu Dhabi. 
	10-01-2007 to 13-02-2007
	Mech, Fitter


	· .
	M/s. Stolt Offshore (ETPM) at Jacson-1 Barge, Sanha Condensate Project, Cabinda Field, ANGOLA. WEST AFRICA.
	10-02-2006 to 02-06-2006
	Mech. Tech

	· 
	M/s. Costain co. At ADMA OPCO OFFSHORE, Survival safety training Course, ZWSC  GG2  ABU DHABI.
	11-09-2003 to 26-12-2005
	Mech. Fitter

	· 
	M/s. Trading and Agency Services Ltd. At Ras Gas,  Plant-I & Plant II. Doha Qatar
	05-01-2002 to 09-07-2003
	Mech. Fitter. 

	· 
	M/s. Al Muftah Co. At Nodco Refinery &Qatar Petroleum Shut Down, DOHA QATAR.
	25-08-2001 to 23-10-2001
	Rotary Tech.

	· 
	Costain co.at ADGAS L.N.G Plant 3 das island ABU DHABI.
	05-04-2001 to 06-05-2001
	Mill Wright Fitter.

	· 
	M/s. United Enterprises,AT PETROKEMYA SAUDI ARABIA
	24-09-1998 to 15-07-2000
	Mech. Tech.

	
	M/s. Costain co, At ADGAS LNG Plant, Das Island ABU DHABI 
	26-03-1996 to18-05-1998
	 Mechanical Tech.






































Nature of work	:	Commissioning, Operation, Maintenance Eraction, Construction, Fabrication of Petrochemical, Oil and (LNG) Gas plants also Refiners, Industrial Maintenance Power plant, water Treatment plant, also work in various field and knowledge in Rotary  and Static Equipment clearance checking bore checking, vibration checking, Alignment checking by different method to attend safety meeting etc.
	
	Mechanical Commissioning checklist
	Description Check

1. Prepare commissioning test log sheet for pump trial run
Bearing Temperatures, oil pressure, oil Temperatures, Casingtemperatur Suction pressure , Discharge pressure, Discharge Temperatures, pump speed, power consumed, Flow Rate, vibration levels.
Discharge pressure, Discharge Temperatures, pump speed, power consumed, Flow Rate, vibration levels.
2. Check hot alignment and record on coupling checklist.
3. check all electrical and instrument checklists are completes.
4. Inspect all associated equipment, IC cooler, expansion tank, pumps etc.
5. Flush system and ensure internal cleanliness.
6. Check that all pump have coupling guards in place.
7. check that al non-essential blinds are removed.
8. check that drain valves are closed  and plugs/caps are installed property.
9. check that all Relief valve are installed and in service.
10. check that all safety warning signs are in the proper location and legible.
11. Verify that all permanent and temporary strainers are being installed in correct position.
12. Ensure that safety valves are installed that they are set to the correct pressure as per P and ID.
13. check all pipe work and associated supports are completed and relevant are complete.
14. Check nozzles are correctly aligned and free from strain. 
15. Confirm flanges can e mated with gasket in place without undue bolt stress prior to final tightening.
16. To check the bolts are tighten by the torque wrench. 
17. To check the suction and discharge line are correct or not.
18. To check the rotation of driver equipment like turbine, motors.
19. In short the rotation are correct as per schedule punch list.
20. Counter clock/clock wise as per choice.
21. To check the proper oil grade
22. To check the proper Greece.
23. Punch list raised.

I was involved in checking of rotary equipments, vibration checking by the vibrometors, temperature checking by the thermometers, RPM chocking by the tachometers, balancing checking by the balancing wheel, run-out-check by dial indicators bore check by the bore indicators, gap checking by the filler gauge, Alignment checking by the different method Ex. Rim and Face, Reverse alignment, graphical alignment and laser alignment to check the hot alignment, cold alignment to check the leveling of the surface, also level transfer by theatrical method, to check the degree of fin fan, profiler fan booster compressor fan by degree protector as per schedule etc.

RECIPROCATING COMPRESSOR :-

MAKE -  Ingersoll Rand, Mutsubishi, Thomssen, Single acting, double acting, Single                 
   stage, Double Stage.
· Maintenance Activities in compressor 
· Preventive maintenance and Trouble shooting of compressor.
· Service and repair both suction and discharge valve.
· Removed piston with piston rod for inspection.
· Replace rider ring, piston ring and packing ring also.
· Checked main bearing clearance by using lead wire.
· Checking web deflection also.
· Checking run - out of piston Rod and connecting Rod big end and Small   end bearing clearance.

STEAM TURBINE 
   MAKE :- Semens, Mutsubishi, Fhuji

   Maintenance Activities in Turbine    
· Preventive and Predictive maintenance of Turbine and its auxiliaries.
· Service and repair of throttle valve (Stop valve)
· Replace the rotor because of damage.
· Centering of rotor.
· Surface checked between upper and lower casing by applying blue matching.
· Change stationary blade and inner packing gland also.
· Align Rotor with the gear box.

GEAR BOX 
   MAKE – BHS, Redicon,Lufkin
Maintenance Activities in gear box.
· Checking the back lash and bearing clearance

VALVE 
   Maintenance Activities in valve
· Recondition of valve seats.
· Hydro testing of the valve at the rated pressure.
· Setting the safety valve for poping pressure & reset pressure.

GAS TURBINE 
MAKE :- GENERAL ELECTRIC.            
  [Frame 5,6,7 and 9, 11]
	No. 6001 B                                                RPM = 5094
	Base – 31.810 KW . 32 MW                     Compressor Stage 17
	Fuel – PROCESS GAS                             Compressor turbine stage - 03
Maintenance Activities in gas turbine 
Preventive  maintenance and Trouble shooting gas turbine and its auxiliaries.
· Remove and replace Linear, Flow Sleeve, Transition piece fuel nozzle and cross fire tube.
· After taking the compressor turbine cover off remove and fix new 1st, 2nd and 3rd Stage nozzle.
· Checking blade condition and clearance.
· Clearance and dimension  checking during overhauling in Comp. Turbine, such as axial rotor clearance, first stage nozzle clamp clearance axial seal clearance, tip clearance.
Radial seal clearance etc.
· Checked VIGB busing clearance and backlash.

Centrifugal Compressor
Make :- Demag, Kobe, Kawasaki.
Maintenance Activities in compressor
· Preventive maintenance and Trouble shooting in compressor 
· Before remove rotor bundle first take axial and redial clearance.
· Removed rotor bundle and replace because of damage and worm out.
· Change labyrinth seal and throttle busing also.
· Replace both seals and bearings. 
· Align the compressor with drive machine.

ALIGNMENT 
(1) Ream and face (2) Reverse – graphic (3) Laser Alignment.


CENTRIFUGAL PUMP
   
   	Single Stage ,Two Stage, and Multi Stage
Make:- Worthington, united centrifugal pump (BMW), Sulzer Bingham
Maintenance  Activities in pump 
· Overhauling and performing checking.
· Clearance and dimension checking during overhauling.
· Replacement of Bearing and mechanical seal.
· Check the out of the shaft.

Mechanical Seal   :-  Single coil and multi coil balanced and unbalanced  single and          
                                  double  
Make                     :-  johan crane, Leak proof, Sealol, Durmetalic

Recondition of seal face. 
 
Reciprocating Pumps

· Suction / Discharge Valve Cheking
· Plunger and Cylinder Clearance Checking
· Plunger Packing Checking
· Crank Chamber Checking
· Small end and Big End Bearing Clearance Checking
· Crank Shaft  Main Bearing Checking
BLOWERS 
· Preventive Maintenance and Overhauling
· Check Lobes Condition
· Check Runout of Bearing Area
· Check Mechanical Seal
· Check Helical Gears Condition,Its Backless and Blue Matching for Lobes
· Contact Setting of Timing Gears
· Clearance of Lobes
· Checking of Belt Condition and its Tightnes

Screw Pump
· Run out of Screwshaft
· Bearing and Screw Shaft Clearance Checking
· Replacement of Mechanical Seal and Bearing
· Alignment Checking

STATIC EQUIPMENT EXPERIENCE : -   In working on heat exchanger, Strainer,    
· Cooler, Heater, burner, Fin fan, Valve servicing for hydro testing, vessels, Tower (Column), Drum, Reactor, Commissioning, Grinding, Cutting, Drilling, Threading and all pipe related work. Loading and unloading work and also performing daily routine service of all equipment 
· STORE :     Procedure draws the material from warehouse the material 
· location material stock,
· SAFETY PROCEDURE: Precaution to be taken while carrying Main Testing/Commissioning Of Mechanical Equipments safety clearances permit to work. Familiar with all kind all kind of permit like Hot Work, Cold Work, Confined Space, Vehicles, Excavation Etc…
                                                                                           Yours faithfully
		                                                                  (Patel Raja R.)			 

